\doxysection{gsm\+\_\+48\+\_\+103.\+h}
\label{gsm__48__103_8h_source}\index{include/osmocom/gsm/protocol/gsm\_48\_103.h@{include/osmocom/gsm/protocol/gsm\_48\_103.h}}
\textbf{ Go to the documentation of this file.}
\begin{DoxyCode}{0}
\DoxyCodeLine{1 \textcolor{comment}{/*}}
\DoxyCodeLine{2 \textcolor{comment}{ * This header file captures the set of fixed RTP payload type definitions}}
\DoxyCodeLine{3 \textcolor{comment}{ * specified in 3GPP TS 48.103 (GSM AoIP interface) Table 5.4.2.2.1.}}
\DoxyCodeLine{4 \textcolor{comment}{ */}}
\DoxyCodeLine{5 }
\DoxyCodeLine{6 \textcolor{preprocessor}{\#pragma once}}
\DoxyCodeLine{7 }
\DoxyCodeLine{8 \textcolor{comment}{/* uncompressed speech */}}
\DoxyCodeLine{9 \textcolor{preprocessor}{\#define OSMO\_AOIP\_RTP\_PT\_PCMU           0}}
\DoxyCodeLine{10 \textcolor{preprocessor}{\#define OSMO\_AOIP\_RTP\_PT\_PCMA           8}}
\DoxyCodeLine{11 }
\DoxyCodeLine{12 \textcolor{comment}{/* compressed speech */}}
\DoxyCodeLine{13 \textcolor{preprocessor}{\#define OSMO\_AOIP\_RTP\_PT\_FR1            3}}
\DoxyCodeLine{14 \textcolor{preprocessor}{\#define OSMO\_AOIP\_RTP\_PT\_EFR            110}}
\DoxyCodeLine{15 \textcolor{preprocessor}{\#define OSMO\_AOIP\_RTP\_PT\_HR1            111}}
\DoxyCodeLine{16 \textcolor{preprocessor}{\#define OSMO\_AOIP\_RTP\_PT\_AMR            112}}
\DoxyCodeLine{17 \textcolor{preprocessor}{\#define OSMO\_AOIP\_RTP\_PT\_AMRWB          113}}
\DoxyCodeLine{18 }
\DoxyCodeLine{19 \textcolor{comment}{/* circuit-\/switched data */}}
\DoxyCodeLine{20 \textcolor{preprocessor}{\#define OSMO\_AOIP\_RTP\_PT\_CSD            120     }\textcolor{comment}{/* without redundancy */}\textcolor{preprocessor}{}}
\DoxyCodeLine{21 \textcolor{preprocessor}{\#define OSMO\_AOIP\_RTP\_PT\_CSD\_RED        121     }\textcolor{comment}{/* with    redundancy */}\textcolor{preprocessor}{}}

\end{DoxyCode}
